TC-CARD 软件操作说明
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一、软件安装
1、 双击安装包，得到一个对话框，在对话框中点击【Next】。
[image: G:\A-霞姐-印刷\A-说明书\A-采集卡说明书\内置采集卡说明书\20.21.5.18\TC CARD\图片1.png图片1]
2、弹出第二个对话框，点击【Install】。
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3， 在弹出的第三个对话框中，点击【Finish】。
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安装成功后，需要重启一次电脑。
1， 【来源】
a，检测采集卡是否能出图像。
[image: G:\A-霞姐-印刷\A-说明书\A-采集卡说明书\内置采集卡说明书\20.21.5.18\TC CARD\图片4.png图片4]
上部大画面是主屏，下部小画面是预览，点击预览可以切换主屏。
当路线太多，预览区显示不完整的时候，按住鼠标左键在预览窗口上，可以进行左右拖动。
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b，可以在界面右侧对图像进行一些参数设置。
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2， 【截取】
截取监测画面的图片。
a， 在【截取】界面右侧做一些简单设置。
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b,勾选预览窗口的黄色框。
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c,点击截取按钮，就可以在指定的文件夹中看到截取的图片。
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3， 【录像】
录取监控画面视频。
a,注意下界面右侧设置。
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b， 勾选红色的框。
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c， 点击录像按钮，就可以在指定的文件夹中，看到录制的视频。
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4， 【串流】
目的：将软件中的信号推到指定平台进行直播。
本次用【目睹直播】平台进行举例串流。
a， 【注册】-【登录】进入【首页】，然后点击【新建直播频道】。
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b，操作完成确定之后，会得到一个页面，点击【专业设备直播】，会得到直播推流地址。
[image: G:\A-霞姐-印刷\A-说明书\A-采集卡说明书\内置采集卡说明书\20.21.5.18\TC CARD\图片16.png图片16]

c,【重点】复制这个链接，将链接分成两部分。
将【watch/】与其之前的内容，粘贴到【串流URL】，将【watch/】之后的内容，粘贴到【串流密钥】。
注意：【串流协议】选择【RTMP】
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（设置完成不要忘记点击【设定】。）

d,点击【串流】。
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e,进入目睹平台，已经在直播了。
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Welcome to the InstaliShield Wizard for
TC_CARD

The Instalishield(R) Wizard wilnstall TC_CARD on your
computer. To continue, cick Next.

WARNING: This programis protected by copyright law and
international reatis.
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3 TC_CARD - InstallShield Wizard

Ready to Install the Program
The wizard i ready to begi installaton.

ClckInstal o begin the instalation.

If you want to review or change any of your installation settings, cck Back. Cick Cancel to
exit the wizerd.
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Instalishield Wizard Completed

The InstaliShield Wizard has successfully installed TC_CARD.
Clck Finsh to exitthe wizard.
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